i28H0

            From the replicator's personal b-log:
            Reincarnations exists.
            Instance cache is not inherited.

Ideal Circuits Simulator -- idealCircuit
----------------------------------------

  http://ic.sidelinesoft.com/downloads/ic.zip

<<
idealCiruit is an analog circuit simulator working with true ideal components.. Students can simulate exactly the same schematics they see in the textbooks.
>>

YouTube tutorials

  Your first schematic in 3 minutes
    https://www.youtube.com/watch?v=H5biAjdH66Q
  All about schematic
    https://www.youtube.com/watch?v=MLiGF0b72F4
  All about transient
    https://www.youtube.com/watch?v=Bph5jwJD7lI
  All about AC
    https://www.youtube.com/watch?v=ZQKPc80agb8

Quick Notes:
............

  + Click component edge or wire edge to place the ground:  <|-  V  -|>

  + Oscilloscope channel is known as "Probe".

  + [ |E]  Separate traces on the Right Toolbar.

Succesful stories:
..................

  1. AC is "программа частотного анализа линейных схем" (back to 1975).
     Weakly tied worlds: digital, analog, switches, UHF, trancient
     (time), AC.

  2. logical.ic example

  3. Logic generator paired with logic controlled switch.

  4. In case we already know how to behave (from real world) there is not much use of simulation. But what if we try something unexpected -- hacker's dream (exploit):

                     -----/\/\/---+---/\/\/-------
  V1=sin(t) r1  gnd               |   \
  R1=1K     r1  +oa                --|+\
  R2=2K     out +oa                  |  >-- blue pill (Matrix, 1999)
  OA        +oa -oa           GND  --|-/
  -oa=GND                             /

Walking through the walls? That's easy.. To be fair, this is so called botanic error -- everything is fine in ideal world..

Right Toolbar:
..............

  Horiz. fit the screen
  <-->   zoom in
  -><-   zoom out
  Vert.  fit the screen
  -v-^-  zoom in
  --x--  zoom out
  <v^>   HV fit the screen
  [ |E]  Separate traces    <<<<<<<<

Categories:

+--------------+-----------+-------------+-----------------+----------+
| Probe:       | voltmeter | amperemeter | +1*0            |          |
|              |           |             |                 |          |
| RCL:         | resistor  | capacitor   |  inductor       |   +1*1   |
|              |           |             |                 |          |
|              |           |             |                 |          |
| Diode:       | diode     | zener       |  bidirectional  | bridge   |
|              |           |             |  zener          | rectifier|
|              |           |             |                 |          |
| Transistor:  | NPN       | PNP         |  N-FET          | P-FET    |
|              |           |             |                 |          |
| Amplifier:   |Operational| +4*2        |                 |          |
|              | Amplifier |             |                 |          |
|              |           |             |                 |          |
| Sources:     | Voltage   | Current     |  4 controlled:  |          |
|              |           |             |  VCV ICV VCI ICI|          |
|              |           |             |  (ИНУН ИНУТ ИТУТ|          |
|              |           |             |  и ИТУН)        |          |
| Switches:    | +8*3      |             |                 |          |
|              |           |             |                 |          |
| Transformer: | Winding   | +1*4        |                 |          |
|              | (дроссель)|             |                 |          |
|              |           |             |                 |          |
| Logical:     | 14 Gates  | 3 flip-flops| 2 Shmitts       | Own +1*5 |
|              |           |             |                 | Source   |
| Misc:        | Delay     | Sample/Hold | +3*6            |          |
+--------------+-----------+-------------+-----------------+----------+

------
*0) +1 AC-source -- probe?
*1) +1 coupled pair -- more than two windings?
*2) buffer amplifier,
    comparator -- ограничитель,
    differential comparator -- компаратор,
    summing amplifier -- 18+
*3) Switches -- аналоговый и цифровой мир плохо соприкасаются,
    что-то наподобие единой теории поля..
*4) See Examples\rect3.ic
*5) Own source: "Logic" generator (Static, Step, Pulse).
    See Examples\logical.ic
*6) Мир СВЧ это не только "длинная линия\". Математика больше чем "функции\".
------

  PS ..> .\upx.exe ic.exe
  PS ..> bash
  $ cp ic.exe icupx.exe
  $ cat icupx.exe | xxd > icupx.xxd
  $ cat icupx.xxd | xxd -r > icresurrected.exe
  $ ls -l
  -rwxrwxrwx 1 virtu virtu 1395712 May 27  2015 ic.exe
  -rwxrwxrwx 1 virtu virtu  457216 Feb  8 20:31 icresurrected.exe
  -rwxrwxrwx 1 virtu virtu  457216 May 27  2015 icupx.exe
  -rwxrwxrwx 1 virtu virtu 1943168 Feb  8 20:30 ic.xxd
