H3GAG

          Alien -- a-lie-n, N-th lie.

Custom Work
-----------

1. Install Crux 3.3 to HD (https://crux.nu, installation guide is in HandbookL: https://crux.nu/Main/Handbook3-3). Computer (virtualbox) configuration:

  OS:        Linux, Other Linux (64-bit)
  Processor: x64_86, 1CPU [v] Enable PAE/NX
  Video:     16MB
  Storage:   Controller IDE: CDROM
             Controller SATA: HD 8GB
  Network:   NAT network, DHCP, NIC: Intel PRO/1000 MT Desktop (8254OEM)

2. Use PIXEL VM (Debian Jessie x64). Install two virtual serial ports. Bridge them with null cable: Project tty0tty, GitHub (Debianize folder). Test configuration using minicom terminal. 

3. Use PIXEL VM (Debian Jessie x64). Install Python 3.x and Thonny IDE. Fix pip (Thonny breaks pip, try thonny-2.0.7.sh instead of 

  python3 -m pip install --upgrade thonny
  
).

  apt-get install python3 python3-pip
  python3 -m pip install --upgrade pyserial
  python3 -m pip install --upgrade thonny
  python3 -m pip install --upgrade pyserial # now broken #

4. Linux On Arduino Yun: Use PIXEL VM (Debian Jessie x64). Install two virtual serial ports. Bridge them with null cable: Project tty0tty, GitHub (Debianize folder). Test configuration using Python pyserial applications:

  Send:                               Receive:
                                        
  import serial                       import serial  
  import time                         import time  
                                      
  ser = serial.Serial('COM5',9600)    ser = serial.Serial('COM7',9600)  
                                      
  time.sleep(2)                       o = ''  
  while True:                         while True:  
    ser.write('Z'.encode())               if ser.in_waiting :  
    time.sleep(1)                             o = ser.read().decode()  
    ser.write('A'.encode())                   print( o)                  
    time.sleep(1)
  ser.close()
  
5. OpenWRT. Install and test in VirtualBox. See my notes "OpenWRT in VirtualBox" here.

6. OpenLDAP. Client and Server are Ubuntu Zesty machines, everything works (see prebuilt pair "OpenlDAPClientSever-H32.rar" in school Samba share). Add XUbuntu 16.10 client. What happend? Create Admin DAZIBAO for this case.

7. Use Zesty VM (Ubuntu Zesty w custom X, x64). Configure as single SSH user computer: 

  + No users logged in. SSH login prompt:

      login as: virtu
      
  + One user logged in. SSH login prompt:

      Closed (Since 20170316 10:25:00). Please try later.
      
8. RTMP server. Follow:

  How to set up your own private RTMP server using nginx 
    https://obsproject.com/forum/resources
    /how-to-set-up-your-own-private-rtmp-server-using-nginx.50/

9. Streamcast with "motion". Follow

  Streaming webcam with "motion" on Raspberry Pi (Raspbian)
  
    nelus.tpt.edu.ee
    
A. Streamcast with VLC. Follow

  http://xmodulo.com/live-stream-video-webcam-linux.html
  
