201301240915


Выбор варианта: номер варианта остаток (%) от деления нацело (\) порядкового номера по списку на сайте:

  www.tptlive.ee -> inimesed -> õpilased -> põhikooli baasil (PÄEVAÕPE) -> Õpperühm: XX-XX
  
на число вариантов. Например, 39-му номеру по списку в случае пяти вариантов:

   39  \  5 = (7,  4)
   
следует выполнять работу номер 4.


Lab 2. Дисплей.

Варианты:

  0. Сименсметр из гальванометра (Пример 3). Внешнюю часть схемы показать в notepad-e.

  1. Компас на 8 направлений. Направление задается кнопкой (вход). Показывает стрелкой и пишет слово
     
     +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
     | | | | |x|x|x| | | |N|O|O|R|D|-|
     +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
     | | | | |x| |x| | | |O|O|S|T| | |
     +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
     | | |x| | | | | | | | | | | | | |
     +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+
     |x| | | | | | | | | | | | | | | |
     +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+

     Голландский: Noorden, Noord-Oost, 
                  Oost, Zuid-Oost
                  Zuiden, Zuid-West,
                  West, Noord-West
     
  2. Вольтметр из гальванометра (Пример 2). Внешнюю часть схемы показать в notepad-e.
     
  3. Амперметр из гальванометра (Пример 3). Внешнюю часть схемы показать в notepad-e.
     
  4. Омметр из гальванометра (Пример 2). Внешнюю часть схемы показать в notepad-e.
     

Пример 1: при нажатии на вход I1 печатает "HELLO", при отпускании "GOODBYE".

Элементы:

  1. вход.
  
  2. тексты сообщений выбрать ячейку дисплея в режиме "свойства блока", печатать туда "HELLO". инвертировать вход "En" даблкликом мауса.
     
  3. тексты сообщений: выбрать ячейку дисплея в режиме "свойства блока", печатать туд а "GOODBYE".         
  
  4. Соединить 1 (out) -> 2 (enable), 1 (out) -> 3 (enable).
    
  5. Пустить симуляцию (F3), показать работу.


Пример 2: отображает цифрой значение на аналоговом входе

Элементы:

  1. аналоговый вход.
  
  2. аналоговый усилитель.
  
  3. Состояние 1 (высокий уровень)
  
  4. тексты сообщений: назначение сообщений - дисплей модуля LOGO!. Выбрать верхнюю левую ячейку дисплея в режиме "свойства блока", перетащить туда (drag'n'drop) Ax с усилением.
     
  5. Соединить 1 (out) -> 2 (ax), 3 (out) -> 4 (en)
  
  6. Пустить симуляцию (F3), показать работу.


Пример 3: отображает полоской значение на аналоговом входе

Элементы:

  1. аналоговый вход.
  
  2. аналоговый усилитель.
  
  3. Состояние 1 (высокий уровень)
  
  4. Общее меню: 
  
     Файл -> Настройка текстов сообщений... ->
      
       [x] Установить новые функции
  
  5. тексты сообщений: назначение сообщений - дисплей модуля LOGO!. Выбрать верхнюю левую ячейку дисплея в режиме "свойства блока", перетащить туда (drag'n'drop) Ax с усилением. Нажать бар: oС [||||||    ] Ai
     
        Параметры: B001 [аналоговый усилитель]
        Текущее значение блока: Ax с усилением
        Мин. значение: 0  Макс. значение: 1000
        Настройка параметров столбца
        Направление (*) Горизонтальная ( ) Вертикальная
        Ширина: 12   Высота: 1
     
  6. Соединить 1 (out) -> 2 (ax), 3 (out) -> 5 (en)
  
  6. Пустить симуляцию (F3), показать работу.


----------
  
Приложение А. Отображаемые параметры и блоки.

  B009 [On-Delay]                    
    Current Time c
    On-Delay p
    Remaining Time c
    
  B010 [Off-Delay]                   
    Current Time c
    Off-Delay p
    Remaining Time c
    
  B011 [On-/Off-Delay]               
    Current Time c
    On-Time (TH) p
    Off-Time (TL) p
    On-Time Remaining (TH) c
    Off-Time Remaining (TL) c
    
  B012 [Retentive On-Delay]          
    Current Time c
    On-Delay p
    Remaining Time c
    
  B013 [Wiping relay (pulse output)] 
    Current Time c
    Off-Time (TL) p
    Off-Time Remaining (TL) c
    
  B014 [Edge triggered wiping relay] 
    Current Time c
    Pulse Width (TH) p
    Interpulse Width (TL) p
    Pulse Width Remaining (TH) c
    Interpulse Width Remaining (TL) c
    
  B015 [Asyncronous Pulse Generator] 
    Current Time c
    Pulse Width (TH) p
    Interpulse Width (TL) p
    Pulse Remaining c
    Interpulse Remaining c
    
  B016 [Random Generator]            
    Max. On Delay (TH) p
    Max. Off Delay (TL) p
    Max. On Delay (TH) Remaining
    Max. Off Delay (TL) Remaining
    
  B017 [Stairway lighting switch]    
    Current Time c
    Off-Delay p
    Pre-warning time (T!)
    Pre-warning period (T!L)
    Off-Delay Remaining c
    Pre-warning time (T!) Remaining c
    Pre-warning period (T!L) Remaining c
    
  B018 [Multiple function switch]    
    Current Time c
    Off-Delay Time (T) p
    Permanent Light (TL) p
    Pre-warning time (T!)
    Pre-warning period (T!L)
    Off-Delay Time (T) Remaining c
    Pre-warning time (T!) Remaining c
    Pre-warning period (T!L) Remaining c
    
  B019 [Weekly Timer]                
    Weekday1 p
    On Time1 p
    Off Time1 p
    Weekday2 p
    On Time2 p
    Off Time2 p
    Weekday3 p
    On Time3 p
    Off Time3 p
    
  B020 [Yearly Timer]                
    On Time (TH) p
    Off Time (TL) p
    
  B021 [Astronomical clock]          
    Longitude p
    Lattitude p
    Time Zone (E+; W-) p
    Sunrise Time c
    Sunset Time c
    
  B022 [Stopwatch]                   
    Time Base p
    Current time c
    Lap Time c
    Output time c
    
  B023 [Up/Down counter]             
    Counter cp
    On Threshold p
    Off Threshold p
    Start Value p
    
  B024 [Hours counter]               
    Maintenance Interval (MI)
    Time-to-go (MN) c
    Total time (OT)
    MI - hour:minute p
    MN - hour:minute c
    OT - hour:minute c
    
  B025 [Threshold trigger]           
    Frequency c
    On Threshold p
    Off Threshold p
    
  B026 [Mathematic instruction]      
    Aq amplified c
    V1 p
    V2 p
    V3 p
    V4 p
    
  B027 [Analog Comparator]           
    On p
    Off p
    Gain
    Offset
    Ax, amplified c
    Ay, amplified c
    Ax (amplified) - Ay (amplified) c
    
  B028 [Analog threshold trigger]    
    On p
    Off p
    Gain
    Offset
    Ax, amplified c
    
  B029 [Analog Amplifier]            
    Gain
    Offset
    Ax, amplified c
    
  B030 [Analog watchdog]             
    Gain
    Offset
    Aen (comparison value) c
    Ax, amplified c
    Threshold 1(+) p
    Threshold 2(-) p
    
  B031 [Analog differential trigger] 
    On p
    Differential p
    Gain
    Offset
    Ax, amplified c
    Off
    
  B032 [Analog MUX]                  
    Aq amplified c
    V1 (S1=0; S2=0) p
    V2 (S1=0; S2=1) p
    V3 (S1=1; S2=0) p
    V4 (S1=1; S2=1) p
    
  B033 [Analog Ramp]                 
    Gain
    Offset
    Current level c
    Level 1 (L1) p
    Level 2 (L2) p
    Largest output value p
    Start/Stop offset p
    Speed of change p
    
  B034 [PI controller]               
    Gain
    Offset
    Smallest process value
    Largest process value
    Set value (SP) p
    Controller amplification (KC) p
    Integration time (TI) p
    Manual output (Mq) p
    Aq c
    PV, amplified (c)
    
  B035 [PWM]                         
    Periodic time p
    Gain
    Offset
    Ax, amplified (current period) c
    
  B036 [Analog filter]               
    Number of samples p
    Ax c
    Aq c
    
  B037 [Max/Min]                     
    Mode p
    Ax c
    Minimum value c
    Maximum value c
    Aq c
    
  B038 [Average Value]               
    Sampling time p
    Number of samples p
    Ax c
    Aq c
    
  B042 [Softkey]                     
    Status cp
    
  B044 [math. instr. error detect ]  
    Referenced math. instr. block
    Overflow c
    Zero division c
  