+74HC00  4  quad 2-input NAND gate
 74HC02  4  quad 2-input NOR gate
+74HC04  6  hex inverter
+74HC08  4  quad 2-input AND gate
+74HC32  4  quad 2-input OR gate
 74HC42  1  BCD to decimal decoder
+74HC74  2  dual D positive edge triggered flip-flop, asynchronous preset and clear
 74HC86  4  quad 2-input XOR gate
 74XX90  1  decade counter (separate divide-by-2 and divide-by-5 sections)
 74XX92  1  divide-by-12 counter (separate divide-by-2 and divide-by-6 sections)
 74XX93  1  4-bit binary counter (separate divide-by-2 and divide-by-8 sections)
74HC138  1  3 to 8-line decoder/demultiplexer, inverting outputs
74HC151  1  8-line to 1-line data selector/multiplexer
74HC164  1  8-bit parallel-out serial shift register, asynchronous clear
74HC165  1  8-bit serial shift register, parallel load, complementary outputs
74HC191  1  synchronous presettable up/down binary counter
74HC273  1  8-bit register, asynchronous clear
74HC573  1  octal D-type transparent latch, three-state outputs
74HC574  1  octal D-type edge-triggered flip-flop, three-state outputs
74HC595  1  8-bit shift registers, output latches, three-state parallel outputs

+ my selection.

  https://en.wikipedia.org/wiki/List_of_7400_series_integrated_circuits

74HC00, 74HC08, 74HC32, 74HC86       74HC74

       ----U----                        ----U----
    1 | 1a  Vcc | 14                 1 o 1RD Vcc | 14
    2 | 1b   4b | 13                 2 | 1D  2RD o 13
    3 | 1Y   4a | 12                 3 | 1CP  2D | 12
    4 | 2a   4Y | 11                 4 o 1SD 2CP | 11
    5 | 2b   3b | 10                 5 | 1Q  2SD o 10
    6 | 2Y   3a |  9                 6 o 1Q   2Q |  9
    7 | GND  3Y |  8                 7 | GND  2Q o  8
       ---------                        ---------

    74HC02                           74HC273

       ----U----                        ----U----
    1 | 1Y  Vcc | 14                 1 o MR  Vcc | 20
    2 | 1a   4Y | 13                 2 | Q0   Q7 | 19
    3 | 1b   4b | 12                 3 | D0   D7 | 18
    4 | 2Y   4a | 11                 4 | D1   D6 | 17
    5 | 2a   3Y | 10                 5 | Q1   Q6 | 16
    6 | 2b   3b |  9                 6 | Q2   Q5 | 15
    7 | GND  3a |  8                 7 | D2   D5 | 14
       ---------                     8 | D3   D4 | 13
                                     9 | Q3   Q4 | 12
    74HC04                          10 | GND  CP | 11
                                        ---------
       ----U----
    1 | 1a  Vcc | 14                 74HC573(LE), 74HC574(CP)
    2 | 1Y   6a | 13
    3 | 2a   6y | 12                    ----U----
    4 | 2Y   5a | 11                 1 o OE  Vcc | 20
    5 | 3a   5Y | 10                 2 | D0   Q0 | 19
    6 | 3Y   4a |  9                 3 | D1   Q1 | 18
    7 | GND  4Y |  8                 4 | D2   Q2 | 17
       ---------                     5 | D3   Q3 | 16
                                     6 | D4   Q4 | 15
    74HC595                          7 | D5   Q5 | 14
                                     8 | D6   Q6 | 13
       ----U----                     9 | D7   Q7 | 12
    1 | Q1  Vcc | 16                10 | GND  LE | 11
    2 | Q2   Q0 | 15                    ---------
    3 | Q3   DS | 14
    4 | Q4   OE o 13
    5 | Q5 STCP | 12
    6 | Q6 SHCP | 11
    7 | Q7   MR o 10
    8 | GND Q7S |  9
       ---------




























    74