GCBJF

                "Peter had seen many tragedies,
                 but he had forgotten them all."
                -- J.M. Barrie, Peter Pan

Burning Arduino UNO R3 Bootloaders
----------------------------------

1: Burning fuses with Atmel Studio 7.0, Pololu 1300 (STK500 emulation)

  Tools -> Add target
    Select tool: STK500
    Select Serial Port: COMx

  Tools -> Device Programming
    Tool: STK500/COMx
    Device: ATMEGA328P
    Interface: ISP
    Device Signature: 0x1E950F
    Target Voltage: 4.8V

    ISP Clock: 57.6KHz
    Fuses:
      EXTENDED BODLEVEL: Brown-out detection at VCC=2.7V
      HIGH.RSTDISBL: [ ]
      HIGH.DWEN:     [ ]
      HIGH.SPIEN:    [v]
      HIGH.WDTON:    [ ]
      HIGH.EESAVE:   [v] !SET!
      HIGH.BOOTSZ:   Boot Flash size=256 words start address=$3F00
      HIGH.BOOTRST:  [v] !SET!
      LOW.CKDIV8     [ ] RESET
      LOW.CKOUT      [ ]
      LOW.SUT_CKSEL: Ext... Crystal Osc. 8.0- MHz;
                     Start-up time PWRDWN/RESET: 16K CK/14 CK + 65ms
                     EXTXOSC_8MHZ_XX_16KCK_14CK_65MS

    Lock Bits:
      LOCKBIT.LB     No memory lock features enabled
      LOCKBIT.BLB0   No lock on SPM and LPM in Application Section
      LOCKBIT.BLB1   LPM and SPM prohibited in Boot Section

    Memories:
      Flash (32KB)
        C:\Program Files (x86)\Arduino\hardware\arduino\avr
          \bootloaders\optiboot\optiboot_atmega328.hex

  :107E0000112484B714BE81FFF0D085E080938100F7
  :107E100082E08093C00088E18093C10086E0809377
  :107E2000C20080E18093C4008EE0C9D0259A86E02C
  :107E300020E33CEF91E0309385002093840096BBD3
  :107E4000B09BFECF1D9AA8958150A9F7CC24DD24C4
  :107E500088248394B5E0AB2EA1E19A2EF3E0BF2EE7
  :107E6000A2D0813461F49FD0082FAFD0023811F036
  :107E7000013811F484E001C083E08DD089C08234E0
  :107E800011F484E103C0853419F485E0A6D080C0E4
  :107E9000853579F488D0E82EFF2485D0082F10E0AE
  :107EA000102F00270E291F29000F111F8ED06801E7
  :107EB0006FC0863521F484E090D080E0DECF843638
  :107EC00009F040C070D06FD0082F6DD080E0C81688
  :107ED00080E7D80618F4F601B7BEE895C0E0D1E017
  :107EE00062D089930C17E1F7F0E0CF16F0E7DF06D8
  :107EF00018F0F601B7BEE89568D007B600FCFDCFD4
  :107F0000A601A0E0B1E02C9130E011968C91119780
  :107F100090E0982F8827822B932B1296FA010C0160
  :107F200087BEE89511244E5F5F4FF1E0A038BF0790
  :107F300051F7F601A7BEE89507B600FCFDCF97BE46
  :107F4000E89526C08437B1F42ED02DD0F82E2BD052
  :107F50003CD0F601EF2C8F010F5F1F4F84911BD097
  :107F6000EA94F801C1F70894C11CD11CFA94CF0C13
  :107F7000D11C0EC0853739F428D08EE10CD085E9AC
  :107F80000AD08FE07ACF813511F488E018D01DD067
  :107F900080E101D065CF982F8091C00085FFFCCF94
  :107FA0009093C60008958091C00087FFFCCF809118
  :107FB000C00084FD01C0A8958091C6000895E0E648
  :107FC000F0E098E1908380830895EDDF803219F02E
  :107FD00088E0F5DFFFCF84E1DECF1F93182FE3DFCA
  :107FE0001150E9F7F2DF1F91089580E0E8DFEE27F6
  :047FF000FF270994CA
  :027FFE00040479
  :0400000300007E007B
  :00000001FF

Links
-----

1. ATMEGA328P-PU как замена Arduino
   http://mysku.ru/blog/aliexpress/22070.html

2. Using Advanced Features of Atmel Studio -- Fuses
   https://www.pololu.com/docs/0J36/3.b.2

2. USBASP & AVRDUDE: Reading fuse bits
   https://rajeshkovvuri.wordpress.com/2012/06/01
         /usbasp-avrdude-reading-fuse-bits/